|  |  |  |  |
| --- | --- | --- | --- |
| **Operator name**:  | **IT.AOC.** | **A/C type:**  | **Location:**  |
| * Implementing Rule reference: (EU) 965/2012 as amended
 | Y: Applicable N: not applicable |
| **Reference** | **Subject** | Y | N | DOCUMENTATION’S REFERENCE REF |
| 1. **GENERAL**
 |
| ARO.OPS.200 | *The airplane is eligible for SET-IMC operations by AFM or other technical document* |  |  |  |
| SPA.SET-IMC.105AMC4 ARO.OPS.200 | *The maintenance and operational procedures*  |  |  |  |
| *flight crew composition and a training/checking are established* *and complies with the applicable requirements of Subpart FC of Part-ORO and Subpart L (SET-IMC) of Part-SPA* |  |  |  |
| *The operator has adequately assessed the risks of the intended operations included in OMA Cap.8.1.13 (AMC3 ORO.MLR.100)* *including the determination of an acceptable risk period if intends to make use of it.* |  |  |  |
| *Operator’s safety performance and experience ensure that the intended safety level is achieved* |  |  |  |
| SPA.SET-IMC.105AMC1 SPA.SET-IMC.105(b) | *The operator achieves and maintains an acceptable level of power plant reliability by reviewing its engine-trend-monitoring programme and propulsion reliability programme, which are established in accordance with Annex I (Part-M) to Regulation (EU) No 1321/2014.* |  |  |  |
| AMC4 ARO.OPS.200 | *Observation of a validation flight, simulating the proposed operation in the aeroplane, has been carried out before an approval is granted* |  |  |  |
| *Observation flight includes flight planning and preflight procedures, as well as a demonstration of simulated emergency procedures in simulated IMC/night:**(a) total failure of the propulsion system; and**(b) total loss of normally generated electrical power.* |  |  |  |
| SPA.SET-IMC.105(a)AMC1 SPA.SET-IMC.105(a) | *Evidence that* *an acceptable level of turbine engine reliability is achieved in service by the world fleet for the particular airframe-engine combination* |  |  |  |
| SPA.SET-IMC.105(d) | *Operating procedures established by the operator specifying:** *equipment, its operating limitations and MEL entries,*
* *flight planning, normal procedures contingency procedures, including procedures following a propulsion system failure,(well as forced landing procedures in all weather conditions)*
* *monitoring and incident reporting.*
 |  |  |  |
| SPA.SET-IMC.105(e) | *Safety Risk Assessment, including the determination of an acceptable risk period if the operator intends to make use of it.(GM2 SPA.SET-IMC.105(d)(2))* |  |  |  |
| GM2SPA.SET-IMC.105(d)(2) | *A safety risk assessment for a specific route must remain below the target fatal accident rate of 1.3 × 10-6, splitting the proposed flight into appropriate segments* |  |  |  |
| AMC3 ORO.MLR.100 | *Procedures included in OMA Cap.8.1.13*  |  |  |  |
| AMC2 SPA.SET-IMC.105(c) | *The minimum crew*  |  |  |  |
| 1. **TRAINING PROGRAMME**
 |
| AMC1 SPA.SET-IMC.105(c) | *Training and checking programme and sillabi i.a.w. sub-part ORO.FC.* |  |  |  |
| *Additional training & checking elements included in following phases:* |  |  |  |
| *a)* ***Conversion training*** *as for AMC1 ORO.FC.220 + item in AMC1 SPA.SET*  *IMC.105(c)*, *point (a)* |  |  |  |
| *b)****Conversion checking*** *(OPC at completion of training ) (OPC ), as for AMC1*  *ORO.FC.230(b)(1)(i) + item in AMC1 SPA.SET-IMC.105(c),* *point (b)* |  |  |  |
| *d)* ***Recurrent training****, as for AMC1 ORO.FC.230(a) + items AMC1SPA.SET*  *IMC.105(c)*, *point (a)* |  |  |  |
| *e)* ***Recurrent checking*** *(OPC ), as for AMC1 ORO.FC.230(b)(1)(i) + item in AMC1*  *SPA.SET-IMC.105(c),* *point (e)* |  |  |  |
| AMC1 SPA.SET-IMC.105(c) | *SET-IMC conversion training and checking is conducted on FFS or FSTD is if available* |  |  |  |
| *RT session and OPCs are conducted in a suitable FFS or FSTD, where available* |  |  |  |
| 1. **FLIGHT PLANNING PROCEDURES**
 |
| AMC1 SPA.SETIMC.105(d)(2) | *Planning procedures are established to ensure that the routes and cruising altitudes are selected so as to have a landing site within gliding range.* |  |  |  |
| *The operator ensure that, except for the take-off and landing, when a risk period is planned, there is a possibility to glide to a non-congested area.* |  |  |  |
| *The total duration of the risk period (1) per flight should not exceed 15 min, with exceptions* |  |  |  |
| *The operator has established criteria for the assessment of each new route based on considerations report at point (c)* |  |  |  |
| *Any selected landing site (2) have been assessed as acceptable for carrying out a safe forced landing with a reasonable expectation of no injuries to persons in the aeroplane or ground* |  |  |  |
| *Landing sites suitable for a diversion/forced landing are programmed into the navigation system so that track and distance are immediately available* |  |  |  |
| *None of these preprogrammed positions are altered in-flight* |  |  |  |
| *Departure, Arrival, En route procedure guarantee that the flight path allows, the aeroplane to land on a landing site in the event of power loss* |  |  |  |
| AMC1 SPA.SETIMC.105(d)(4) | *When a risk period is used during take-off or landing, the contingency procedures include appropriate information for the crew on the path to be followed after an engine failure* |  |  |  |
| 1. **EQUIPMENT**
 |
| SPA.SET-IMC.110 | * *two separate electrical generating systems*
 |  |  |  |
| * *two attitude indicators, powered from independent sources;(2nd can be the backup/stby) AMC1 SPA.SET-IMC.110(b)*
 |  |  |
| * *a shoulder harness/safety belt with a diagonal shoulder strap for each passenger seat*
 |  |  |
| * *airborne weather-detecting equipment (AMC1 SPA.SET-IMC.110(d))*
 |  |  |
| * *in a pressurised aeroplane, sufficient supplemental oxygen for all occupants*
 |  |  |
| * *an RNAV system with the positions of landing sites and providing lateral guidance on RNP Aprch (GNSS) (AMC1 SPA.SET-IMC.110(f))*
 |  |  |
| * *a radio altimeter*
 |  |  |
| * *a landing light, capable of illuminating the touchdown point on the power-off glide path from 200 ft away (GM1 SPA.SET-IMC.110(h))*
 |  |  |
| * *an emergency electrical supply system*
 |  |  |
| * *an ignition system automatic or manual for flying in visible moisture;*
 |  |  |
| * *a means of continuously monitoring the power train lubrication system*
 |  |  |
| *-an emergency engine power control device (AMC1 SPA.SET-IMC.110(l))* |  |  |
| **Remarks (state non conformities with reference to RMK ref. no.):** |

|  |  |
| --- | --- |
| **NOMINATED PERSON FLIGHT OPERATIONS** **NOMINATED PERSON CREW TRAINING** **COMPLANCE MONITORING MANAGER**  | \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |